# Unit preferences for categories of data.
# Units will be diplayed exactly as entered.

PCB2PCB_DISTANCE                cm
PCB_DISTANCE                    cm
ALTITUDE                        m
TEMPERATURE                     degC
THERM_CONDUCTANCE               w/cm-degC
THERM_CONDUCTIVITY              w/cm-degC
VOLTAGE                         V
NOISE_VOLTAGE                   mV
DIODE_VOLTAGE                   V
VELOCITY                        m/s
PROP_VELOCITY                   mil/ns
ELEC_CONDUCTIVITY               mho/cm
ETCH_THICKNESS                  mil
FAILURE_RATE                    fpmh
CAPACITANCE                     pF
IMPEDANCE                       ohm
PROP_DELAY                      ns
CLOCK_SKEW                      ps
ETCH_RESISTANCE                 mOhm
RESISTANCE                      Ohm
INDUCTANCE                      nH
THERM_RESISTANCE                degC/w
PRESSURE                        atm
PERCENTAGE                      %
TIME                            s
CLOCK_FREQUENCY                 MHz
TRACE_ROUGHNESS                 um

# Units conversion mapping data.
# One numeric scaling prefix is allowed per mapping.
# A numeric suffix indicates exponentiation (eg. CM3 for centimeter-cubed).
# All units must ultimately map to one of the following fundamental units:
#
# METER  RADIAN  SECOND  DEGC  GRAM  COULOMB DIMENSIONLESS

P				PS
N				NS
M                               METER
MILE                            5280FEET
FURLONG                         0.125MILE
FEET                            0.3048METER
FOOT                            FEET
FT                              FEET
'                               FEET
INCH                            0.0254METER
IN                              INCH
INS                             INCH
"                               INCH
MIL                             0.001INCH
MICRON                          UMETER
SMOOT                           67INCH
SMOOTS                          SMOOT
OZ.CU                           1.44MIL
OZ.FL                           29.57353CC
GALLON                          128OZ.FL
GAL                             GALLON
CC                              CM3
LITER                           1000CC
L                               LITER
MPH                             MILE/HOUR
RAD                             RADIAN
DEGREE                          0.017453292519943295769222RADIAN
DEGREES                         DEGREE
DEG                             DEGREE
SEC                             SECOND
S                               SECOND
MINUTE                          60SECOND
MIN                             MINUTE
HOUR                            3600SECOND
HR                              HOUR
DAY                             24HOUR
FORTNIGHT                       14DAY
C                               DEGC
DEGF                            0.555555555555555555555555555555DEGC
F                               DEGF
G                               GRAM
GF                              0.00980665NEWTON
POUND                           453.59237GRAM
LB                              POUND
LBS                             POUND
LBF                             32.174POUND-FEET/SECOND2
OUNCE                           28.349523125GRAM
OZF                             32.174OUNCE-FEET/SECOND2
DYNE                            0.00001NEWTON
PSI                             LBF/INCH2
PASCAL                          NEWTON/METER2
PA                              PASCAL
NEWTON                          KGRAM-METER/SECOND2
VOLT                            NEWTON-METER/COULOMB
V                               VOLT
VOLTS                           VOLT
AMPERE                          COULOMB/SEC
A                               AMPERE
AMP                             AMPERE
AMPS                            AMPERE
WEBER                           NEWTON-METER/AMPERE
HENRY                           WEBER/AMPERE
H                               HENRY
WATT                            VOLT-AMPERE
W                               WATT
WATTS                           VOLT-AMPERE
FARAD                           COULOMB/VOLT
F                               FARAD
JOULE                           WATT-SECOND
J                               JOULE
BTU                             1055.05585262JOULE
OHM                             VOLT/AMPERE
OHMS                            OHM
MHO                             AMPERE/VOLT
MHOS                            MHO
SEIMEN                          MHO
HORSEPOWER                      550FEET-LBF/SECOND
HP                              HORSEPOWER
CPS                             CYCLE/SECOND
HZ                              CYCLE/SECOND
MHZ                             MEGHZ
PERCENT                         0.01DIMENSIONLESS
%                               PERCENT
ATM                             14.696PSI
# a LINE is an isotherm line, required for the Thermal Parameters Form
LINE                            DIMENSIONLESS
CYCLE                           DIMENSIONLESS
FAILURE                         DIMENSIONLESS
FPMH                            FAILURE/MEGHOUR
PPHH                            PERCENT/100HOUR
ACRE                            43560FT2
# standard database units
MILS                            0.001INCH
INCHES                          0.0254METER
MILLIMETERS                     0.001METER
CENTIMETERS                     0.01METER
MICRONS                         0.000001METER
